\documentstyle{article}
\setlength{\topmargin}{-45pt}
\setlength{\oddsidemargin}{0cm}
\setlength{\evensidemargin}{-0cm}
\setlength{\textheight}{24cm}
\setlength{\textwidth}{16cm}

\newcommand{\ind}{\par\hangindent=0.5cm\hangafter=1\noindent}
\newcommand{\indd}{\par\hangindent=1.0cm\hangafter=1\hspace*{0.5cm}}
\newcommand{\idl}{\hspace*{5mm}{\tt IDL>\ }}
\newcommand{\unix}{\hspace*{5mm}{\tt unix\%\ }}
\newcommand{\crmk}{{\bf $<$CR$>$}}
\newcommand{\ssw}{{\tt \$\{SSW\}}}
\newcommand{\norp}{{\tt \$\{NORP\}}}



\begin{document}
\title{Nobeyama Radio Interferometer (NoRI) \\
Analysis Manual
\\
ver. 0.0
}
\author{T. Yokoyama}
\date{July 7, 2000}
\maketitle

%\clearpage
\section{Introduction}

This is a manual for analysis of the data
obtained by Nobeyama Radio Interferometer (NoRI; stop operation in Jul 1992;
Nakajima et al. 1980)

For any questions and requests, please send an e-mail to \\
\bigskip
\hspace*{1cm}{\tt nsro-service@solar.nro.nao.ac.jp}

The latest information on NoRS is updated on NSRO Web site.
The URL is \\
\bigskip
\hspace*{1cm} {\tt http://solar.nro.nao.ac.jp/nori/}\\

\section{How to setup}

\medskip
\noindent
(1) Installation of the {\it SolarSoftware}.

Install the SolarSoftware (SSW).
If this was not installed, please contact your
system manager.
The primary distribution site for SolarSoftware is:
{\tt http://www.lmsal.com/solarsoft/}

\medskip
\noindent
(2) Setup of your personal environment

Include the followings in your environment setup file ({\tt \char126/.cshrc}). \
\
{\tt 
\hspace*{10mm} setenv SSW {\it SSW-directory}\footnote{
{\tt /sgi1/ssw} in NSRO} \\
\hspace*{10mm} setenv SSW\_INSTR ``nori'' \\
\hspace*{10mm} setenv NORS \$\{SSW\}/radio/nori \\ 
\hspace*{10mm} source \$\{SSW\}/gen/setup/setup.ssw \\
\hspace*{10mm} source \$\{NORI\}/setup/setup.nori  \\
}
Note that the enviroment variable {\ssw} can be different
(Ask your system manager)\footnote{In NSRO, it is {\tt /sgi1/ssw}}. 
In case you analyze many kinds of
data at the same time, define SSW\_INSTR as follows, e.g. \\
{\tt
\hspace*{10mm} setenv SSW\_INSTR ``nori sxt nors'' \\
}


\section{Where is the Data ?}

\subsection{Raw Data}

Some raw NoRI data 
are put in the NSRO archive.
You can obtain them by anonymous FTP.

\section{Analysis}

\subsection{Start Analysis}

The NoRI IDL procedures described in this section all depend on the
SolarSoftware (SSW). When you start the analysis, start up
the SSW/IDL as follows:

\unix {\bf sswidl \crmk}

\section{Read the Data}

In order to read the data into IDL session, give the file name as follows: \\
\idl {\bf file='./if911202'} \\
\idl {\bf nori\_rd\_dat,file,index,data \crmk} \\
%
In order to read the data in specified duration: \\
\idl {\bf timerange=['1991-12-2 2:00','1991-12-2 4:00'] \crmk} \\
\idl {\bf nori\_rd\_dat,file,index,data,timerange=timerange \crmk} \\


\section{Plot}

For plotting, \\
\idl {\bf nori\_plot,index(0),data(*,0,0) \crmk} \\

\appendix

\section{NoRS data archive: anonymous FTP}
\label{archive}

The Nobeyama Solar Radio Observatory (NSRO/NAOJ) has prepared
the anonymous FTP server for the NoRS data archive. 
The URL is 

\bigskip
{\tt ftp://nsro-archive.nro.nao.ac.jp/pub/nori}
\bigskip

If you need to transfer a large amount of data ,
please contact

\bigskip
{\tt nsro-service@solar.nro.nao.ac.jp}

We will make and mail a CD-ROM for you.
The network capability in Nobeyama is limited.


\section{Acknowledgement}

We thank the following people.
SolarSoftware is a software package for analysis of Solar
Data on IDL. That is supported under various
NASA contracts (SXT/EIT/MDI/TRACE/YPOP etc.) and is all in
the public domain.
IDL is a product by Research System Inc.

\section*{References}

\noindent
Nakajima et al., "A New 17-GHz Solar Radio Interferometer at Nobeyama",
1980, PASJ, 32, 639


\end{document}
